(kicad_pcb (version 4) (host pcbnew 4.0.6-e0-6349~53~ubuntu16.04.1)
  (general
    (links 132)
    (no_connects 0)
    (area 94.260999 64.923999 259.181427 179.17)
    (thickness 1.6)
    (drawings 19)
    (tracks 780)
    (zones 0)
    (modules 70)
    (nets 40)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu power hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.3)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 1)
    (via_drill 0.8)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 1.5 0.8)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.59 0.45)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 162.052 81.153)
    (visible_elements 7FFFEFFF)
    (pcbplotparams
      (layerselection 0x3ffff_80000001)
      (usegerberextensions false)
      (excludeedgelayer false)
      (linewidth 0.020000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory /home/elektra/MP-Tracker-Production-Files/))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GNDPWR)
  (net 3 +BATT)
  (net 4 "Net-(C3-Pad1)")
  (net 5 "Net-(C4-Pad2)")
  (net 6 "Net-(C5-Pad1)")
  (net 7 VCC)
  (net 8 +3.3V)
  (net 9 "Net-(C8-Pad1)")
  (net 10 "Net-(C10-Pad1)")
  (net 11 "Net-(C11-Pad1)")
  (net 12 "Net-(C12-Pad1)")
  (net 13 "Net-(D1-Pad1)")
  (net 14 "Net-(D1-Pad2)")
  (net 15 VAA)
  (net 16 "Net-(D5-Pad2)")
  (net 17 "Net-(P1-Pad1)")
  (net 18 "Net-(P1-Pad2)")
  (net 19 "Net-(P1-Pad3)")
  (net 20 "Net-(P1-Pad5)")
  (net 21 "Net-(P1-Pad9)")
  (net 22 "Net-(Q3-Pad1)")
  (net 23 "Net-(Q3-Pad3)")
  (net 24 "Net-(R1-Pad2)")
  (net 25 "Net-(R3-Pad2)")
  (net 26 "Net-(R7-Pad2)")
  (net 27 "Net-(R8-Pad2)")
  (net 28 "Net-(R11-Pad2)")
  (net 29 "Net-(R19-Pad1)")
  (net 30 "Net-(R26-Pad2)")
  (net 31 "Net-(C16-Pad1)")
  (net 32 "Net-(C17-Pad1)")
  (net 33 "Net-(C18-Pad1)")
  (net 34 "Net-(D4-Pad2)")
  (net 35 "Net-(P2-Pad1)")
  (net 36 "Net-(R19-Pad2)")
  (net 37 "Net-(R25-Pad1)")
  (net 38 "Net-(R31-Pad1)")
  (net 39 "Net-(P1-Pad7)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.3)
    (via_dia 1)
    (via_drill 0.8)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3.3V)
    (add_net "Net-(P1-Pad3)")
    (add_net VAA)
  )
  (net_class Medium ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 1)
    (via_drill 0.8)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +BATT)
    (add_net GNDPWR)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C16-Pad1)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(C18-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad5)")
    (add_net "Net-(P1-Pad7)")
    (add_net "Net-(P1-Pad9)")
    (add_net "Net-(P2-Pad1)")
    (add_net "Net-(Q3-Pad1)")
    (add_net "Net-(Q3-Pad3)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R19-Pad1)")
    (add_net "Net-(R19-Pad2)")
    (add_net "Net-(R25-Pad1)")
    (add_net "Net-(R26-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R31-Pad1)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(R8-Pad2)")
    (add_net VCC)
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 1)
    (via_dia 1)
    (via_drill 0.8)
    (uvia_dia 0.8)
    (uvia_drill 0.6)
  )
  (net_class Small ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 1)
    (via_drill 0.8)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 596CBCA7)
    (at 138.049 100.965 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at -3.2004 -0.0762 270) (layer F.SilkS))
    (fp_text value 68p (at -0.2032 2.0066 90) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 596CBE5A)
    (at 103.1875 94.0435 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 0 -2.1 180) (layer F.SilkS))
    (fp_text value 15p (at 0 -3.5052 180) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 596CBE46)
    (at 103.1875 83.3755)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 15p (at 0.2032 -4.0132) (layer F.SilkS))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SOD-123 (layer F.Cu) (tedit 596CBC48)
    (at 104.013 114.808)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D1 (at 3.7465 0.0381) (layer F.SilkS))
    (fp_text value 1N4148 (at -5.5499 0.3937) (layer F.SilkS))
    (pad 1 smd rect (at -1.635 0) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 1.635 0) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D1-Pad1)"))
  )
  (module Choke_SMD:Choke_SMD_12x12mm_h8mm (layer F.Cu) (tedit 596DF08C)
    (at 126.8349 116.8527)
    (descr "Choke, SMD, 12x12mm 8mm height")
    (tags "Choke, SMD")
    (attr smd)
    (fp_text reference L1 (at -3.8354 -7.4422) (layer F.SilkS))
    (fp_text value 27u (at 0.8636 -7.5692) (layer F.SilkS))
    (pad 1 smd rect (at -4.95046 0) (size 2.90068 5.40004) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D5-Pad2)"))
    (pad 2 smd rect (at 4.95046 0) (size 2.90068 5.40004) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C11-Pad1)"))
    (model Choke_SMD.3dshapes/Choke_SMD_12x12mm_h8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 4 4 4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965 (layer F.Cu) (tedit 591347AD)
    (at 167.64 70.485)
    (descr "Mounting Hole 3.2mm, no annular, M3, DIN965")
    (tags "mounting hole 3.2mm no annular m3 din965")
    (fp_text reference "" (at 0.381 5.715) (layer F.SilkS))
    (fp_text value "" (at 0 3.8) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Power_Integrations:SO-8 (layer F.Cu) (tedit 596CACA2)
    (at 132.1435 72.1995 270)
    (descr "SO-8 Surface Mount Small Outline 150mil 8pin Package")
    (tags "Power Integrations D Package")
    (fp_text reference U4 (at 0 0 270) (layer F.SilkS))
    (fp_text value MC78L033 (at -3.4544 -0.0508 360) (layer F.SilkS))
    (pad 1 smd oval (at -1.905 2.794 270) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 8 +3.3V))
    (pad 2 smd oval (at -0.635 2.794 270) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (pad 3 smd oval (at 0.635 2.794 270) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (pad 4 smd oval (at 1.905 2.794 270) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd oval (at 1.905 -2.794 270) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd oval (at 0.635 -2.794 270) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (pad 7 smd oval (at -0.635 -2.794 270) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (pad 8 smd oval (at -1.905 -2.794 270) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 3 +BATT))
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 596CAFDD)
    (at 144.9832 77.3938)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R22 (at -0.1524 -1.778) (layer F.SilkS))
    (fp_text value 47 (at -0.1524 1.7272) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C16-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 596CBCDF)
    (at 128.9304 95.2754 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R21 (at -0.254 -1.6764 180) (layer F.SilkS))
    (fp_text value 2k35 (at -0.254 -2.6924 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(R19-Pad2)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 596CBE01)
    (at 144.907 90.043)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at -0.2794 -1.4732) (layer F.SilkS))
    (fp_text value 22k (at 8.6614 0.1016) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R11-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x05 (layer F.Cu) (tedit 590891D3)
    (at 111.0615 73.3425 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 2.2987 -2.7559 90) (layer F.SilkS))
    (fp_text value "" (at 1.2065 -4.3815 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(P1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(P1-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(P1-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 +3.3V))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(P1-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GNDPWR))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(P1-Pad7)"))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GNDPWR))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(P1-Pad9)"))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GNDPWR))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x05.wrl
      (at (xyz 0.05 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Choke_SMD:Choke_SMD_12x12mm_h8mm (layer F.Cu) (tedit 596DF09F)
    (at 144.3355 116.7765)
    (descr "Choke, SMD, 12x12mm 8mm height")
    (tags "Choke, SMD")
    (attr smd)
    (fp_text reference L2 (at -0.508 -7.493) (layer F.SilkS))
    (fp_text value "" (at 2.032 -7.747) (layer F.SilkS))
    (pad 1 smd rect (at -4.95046 0) (size 2.90068 5.40004) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 4.95046 0) (size 2.90068 5.40004) (layers F.Cu F.Paste F.Mask)
      (net 3 +BATT))
    (model Choke_SMD.3dshapes/Choke_SMD_12x12mm_h8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 4 4 4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:c_elec_10x10 (layer F.Cu) (tedit 596E05D0)
    (at 151.7015 132.0165 90)
    (descr "SMT capacitor, aluminium electrolytic, 10x10")
    (attr smd)
    (fp_text reference C14 (at 0 -6.35 90) (layer F.SilkS))
    (fp_text value 330u (at 7.0485 3.4925 180) (layer F.SilkS))
    (pad 1 smd rect (at 4.0005 0 90) (size 4.0005 2.4003) (layers F.Cu F.Paste F.Mask)
      (net 3 +BATT))
    (pad 2 smd rect (at -4.0005 0 90) (size 4.0005 2.4003) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (model Capacitors_SMD.3dshapes/c_elec_10x10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 596CBC91)
    (at 131.826 102.616 180)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at -0.1524 -0.0762 180) (layer F.SilkS))
    (fp_text value MC34063 (at 0.3556 -4.7498 180) (layer F.SilkS))
    (pad 1 smd rect (at -2.7 -1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R3-Pad2)"))
    (pad 2 smd rect (at -2.7 -0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (pad 3 smd rect (at -2.7 0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C8-Pad1)"))
    (pad 4 smd rect (at -2.7 1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (pad 5 smd rect (at 2.7 1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(R19-Pad2)"))
    (pad 6 smd rect (at 2.7 0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 7 smd rect (at 2.7 -0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 8 smd rect (at 2.7 -1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R1-Pad2)"))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:c_elec_10x10 (layer F.Cu) (tedit 596CBC0D)
    (at 109.0295 131.3815 90)
    (descr "SMT capacitor, aluminium electrolytic, 10x10")
    (attr smd)
    (fp_text reference C6 (at 3.2385 6.4897 90) (layer F.SilkS))
    (fp_text value 330u (at 0 6.35 90) (layer F.SilkS))
    (pad 1 smd rect (at 4.0005 0 90) (size 4.0005 2.4003) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at -4.0005 0 90) (size 4.0005 2.4003) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (model Capacitors_SMD.3dshapes/c_elec_10x10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:c_elec_10x10 (layer F.Cu) (tedit 596CB013)
    (at 137.1981 131.9911 90)
    (descr "SMT capacitor, aluminium electrolytic, 10x10")
    (attr smd)
    (fp_text reference C13 (at 4.0386 -6.3246 90) (layer F.SilkS))
    (fp_text value 1000u (at 0 6.35 90) (layer F.SilkS))
    (pad 1 smd rect (at 4.0005 0 90) (size 4.0005 2.4003) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at -4.0005 0 90) (size 4.0005 2.4003) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (model Capacitors_SMD.3dshapes/c_elec_10x10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:c_elec_10x10 (layer F.Cu) (tedit 596E05DF)
    (at 151.7015 132.0165 90)
    (descr "SMT capacitor, aluminium electrolytic, 10x10")
    (attr smd)
    (fp_text reference C14 (at 0 -6.35 90) (layer F.SilkS))
    (fp_text value "" (at 7.6835 3.4925 180) (layer F.Fab) hide)
    (pad 1 smd rect (at 4.0005 0 90) (size 4.0005 2.4003) (layers F.Cu F.Paste F.Mask)
      (net 3 +BATT))
    (pad 2 smd rect (at -4.0005 0 90) (size 4.0005 2.4003) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (model Capacitors_SMD.3dshapes/c_elec_10x10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SOD-123 (layer F.Cu) (tedit 596CBDBE)
    (at 149.479 96.266)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D4 (at 3.4544 -0.381) (layer F.SilkS))
    (fp_text value 6V2 (at -4.2164 -0.0254) (layer F.SilkS))
    (pad 1 smd rect (at -1.635 0) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(D4-Pad2)"))
    (pad 2 smd rect (at 1.635 0) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
  )
  (module Choke_SMD:Choke_SMD_12x12mm_h8mm (layer F.Cu) (tedit 596DF0A5)
    (at 144.3355 116.7765)
    (descr "Choke, SMD, 12x12mm 8mm height")
    (tags "Choke, SMD")
    (attr smd)
    (fp_text reference L2 (at -0.508 -7.493) (layer F.SilkS))
    (fp_text value 10u (at 3.7465 -7.5565) (layer F.SilkS))
    (pad 1 smd rect (at -4.95046 0) (size 2.90068 5.40004) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 4.95046 0) (size 2.90068 5.40004) (layers F.Cu F.Paste F.Mask)
      (net 3 +BATT))
    (model Choke_SMD.3dshapes/Choke_SMD_12x12mm_h8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 4 4 4))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 596CBC5A)
    (at 103.5685 121.2215)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 -2.25) (layer F.SilkS))
    (fp_text value BC817-40 (at 0.0635 2.7305) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D1-Pad1)"))
    (pad 3 smd rect (at 0 -0.99822) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:TO-252-2Lead (layer F.Cu) (tedit 596CBC38)
    (at 108.6485 119.6975 270)
    (descr "DPAK / TO-252 2-lead smd package")
    (tags "dpak TO-252")
    (attr smd)
    (fp_text reference Q2 (at 0 -10.414 270) (layer F.SilkS))
    (fp_text value IRFR5303 (at -4.5085 -6.4135 360) (layer F.SilkS))
    (pad 1 smd rect (at -2.286 0 270) (size 1.651 3.048) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 0 -6.35 270) (size 6.096 6.096) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D5-Pad2)"))
    (pad 3 smd rect (at 2.286 0 270) (size 1.651 3.048) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model TO_SOT_Packages_SMD.3dshapes/TO-252-2Lead.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 596CBDA2)
    (at 155.8544 107.061)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q3 (at 2.9464 -0.7112) (layer F.SilkS))
    (fp_text value BC817-40 (at 8.1026 1.143) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(Q3-Pad1)"))
    (pad 2 smd rect (at 0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (pad 3 smd rect (at 0 -0.99822) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(Q3-Pad3)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:TO-252-2Lead (layer F.Cu) (tedit 596CBD6D)
    (at 156.1465 118.6815 270)
    (descr "DPAK / TO-252 2-lead smd package")
    (tags "dpak TO-252")
    (attr smd)
    (fp_text reference Q4 (at 0 -10.414 270) (layer F.SilkS))
    (fp_text value IRFR5303 (at 4.7625 -6.2865 360) (layer F.SilkS))
    (pad 1 smd rect (at -2.286 0 270) (size 1.651 3.048) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(Q3-Pad3)"))
    (pad 2 smd rect (at 0 -6.35 270) (size 6.096 6.096) (layers F.Cu F.Paste F.Mask)
      (net 15 VAA))
    (pad 3 smd rect (at 2.286 0 270) (size 1.651 3.048) (layers F.Cu F.Paste F.Mask)
      (net 3 +BATT))
    (model TO_SOT_Packages_SMD.3dshapes/TO-252-2Lead.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 596CBC9A)
    (at 124.333 103.378 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -2.1 270) (layer F.SilkS))
    (fp_text value 1k (at 0 2.1 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 596CBC6C)
    (at 103.4415 109.5375)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 4K7 (at 0 2.1) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 596CBC75)
    (at 103.378 105.029)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at -2.9972 0.0508) (layer F.SilkS))
    (fp_text value 470R (at 3.7592 0.0508) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R3-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 596CBD99)
    (at 155.829 111.633 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 -2.1 180) (layer F.SilkS))
    (fp_text value 1k (at -2.921 -0.1016 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(Q3-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 596CBDA9)
    (at 154.8384 103.5558)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at -2.6924 -0.1016) (layer F.SilkS))
    (fp_text value 10k (at 3.2512 -0.1016) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +BATT))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(Q3-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 596CBEA5)
    (at 127.7747 86.1187 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at -0.0127 -1.4351 90) (layer F.SilkS))
    (fp_text value 47R (at -0.2159 1.6637 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 +3.3V))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 596CBE76)
    (at 118.4275 91.8235 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 2.0853 0.0381 180) (layer F.SilkS))
    (fp_text value 1k (at -2.1311 0.0381 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(Q3-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(R7-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 596CBEFC)
    (at 125.5395 75.8825 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 2.4765 -0.3175 180) (layer F.SilkS))
    (fp_text value 27k (at -3.1369 -0.4953 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(R8-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 596CBFCE)
    (at 125.5395 73.2155)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at 0.8255 -1.7145) (layer F.SilkS))
    (fp_text value 3k3 (at 1.5875 -2.9845) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(R8-Pad2)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 596CBE99)
    (at 134.9248 91.0082)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R10 (at -0.8128 -1.4732) (layer F.SilkS))
    (fp_text value 1K (at -1.0668 1.4732) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C18-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C10-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 596CBE09)
    (at 144.907 90.043)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at -0.2794 -1.4732) (layer F.SilkS))
    (fp_text value 22k (at 8.6614 0.1016) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R11-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 596CBE1E)
    (at 149.733 90.043)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R12 (at -0.0762 -1.4732) (layer F.SilkS))
    (fp_text value 3k3 (at 7.4422 0.1524) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R11-Pad2)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 596CBDF8)
    (at 144.78 93.98)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R13 (at -0.0508 -1.7526) (layer F.SilkS))
    (fp_text value 10k (at 7.4676 -0.1778) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(D4-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 596CBDF0)
    (at 148.59 93.9546 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R14 (at -0.1016 1.7272 180) (layer F.SilkS))
    (fp_text value 33k (at -7.5692 0.1524 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C12-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(D4-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 596CBEC0)
    (at 138.176 85.598 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R16 (at 0.762 2.3622 180) (layer F.SilkS))
    (fp_text value 6k8 (at 0.8128 1.4986 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 596CBEC9)
    (at 144.018 86.106 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R19 (at 0.762 2.54 270) (layer F.SilkS))
    (fp_text value 10k (at 2.286 0.889 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R19-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(R19-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 596CBCEE)
    (at 134.112 97.282 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R20 (at 0.2032 1.4478 180) (layer F.SilkS))
    (fp_text value 27k (at -0.0508 -1.5494 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(R19-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 596CBE3C)
    (at 124.3584 69.6722 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R25 (at 2.1082 -0.1524 180) (layer F.SilkS))
    (fp_text value 1K (at 3.1242 2.3876 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(R25-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(P2-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58FF793F)
    (at 139.1412 76.5302 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R26 (at -2.0828 0 360) (layer F.SilkS))
    (fp_text value 15k (at 2.1336 -0.1016 360) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +BATT))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(R26-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 596CBEE2)
    (at 128.2725 80.7085)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R27 (at 2.4867 -0.8763) (layer F.SilkS))
    (fp_text value 3k3 (at 2.4867 0.0381) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(R26-Pad2)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8-1EP_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58FF79DA)
    (at 148.8948 83.4644 90)
    (descr "8-Lead Thermally Enhanced Plastic Small Outline (SE) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U2 (at 0.4826 -0.1016 180) (layer F.SilkS))
    (fp_text value TL081 (at -0.6858 -0.1016 180) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R11-Pad2)"))
    (pad 3 smd rect (at -2.7 0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C12-Pad1)"))
    (pad 4 smd rect (at -2.7 1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (pad 5 smd rect (at 2.7 1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 2.7 0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R19-Pad1)"))
    (pad 7 smd rect (at 2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C16-Pad1)"))
    (pad 8 smd rect (at 2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask))
    (model Housings_SOIC.3dshapes/SOIC-8-1EP_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:LQFP-32_7x7mm_Pitch0.8mm (layer F.Cu) (tedit 596CBEEB)
    (at 120.6119 83.1723)
    (descr "LQFP32: plastic low profile quad flat package; 32 leads; body 7 x 7 x 1.4 mm (see NXP sot358-1_po.pdf and sot358-1_fr.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference U3 (at -0.4699 -1.7145) (layer F.SilkS))
    (fp_text value ATMEGA8 (at 8.9281 -5.0673) (layer F.SilkS))
    (pad 1 smd rect (at -4.25 -2.8) (size 1.2 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -4.25 -2) (size 1.2 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -4.25 -1.2) (size 1.2 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (pad 4 smd rect (at -4.25 -0.4) (size 1.2 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 +3.3V))
    (pad 5 smd rect (at -4.25 0.4) (size 1.2 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (pad 6 smd rect (at -4.25 1.2) (size 1.2 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 +3.3V))
    (pad 7 smd rect (at -4.25 2) (size 1.2 0.55) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad2)"))
    (pad 8 smd rect (at -4.25 2.8) (size 1.2 0.55) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 9 smd rect (at -2.8 4.25 90) (size 1.2 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at -2 4.25 90) (size 1.2 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at -1.2 4.25 90) (size 1.2 0.55) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(R7-Pad2)"))
    (pad 12 smd rect (at -0.4 4.25 90) (size 1.2 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at 0.4 4.25 90) (size 1.2 0.55) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(R31-Pad1)"))
    (pad 14 smd rect (at 1.2 4.25 90) (size 1.2 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at 2 4.25 90) (size 1.2 0.55) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(P1-Pad1)"))
    (pad 16 smd rect (at 2.8 4.25 90) (size 1.2 0.55) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(P1-Pad2)"))
    (pad 17 smd rect (at 4.25 2.8) (size 1.2 0.55) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(P1-Pad3)"))
    (pad 18 smd rect (at 4.25 2) (size 1.2 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 19 smd rect (at 4.25 1.2) (size 1.2 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at 4.25 0.4) (size 1.2 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 21 smd rect (at 4.25 -0.4) (size 1.2 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (pad 22 smd rect (at 4.25 -1.2) (size 1.2 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 4.25 -2) (size 1.2 0.55) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(R26-Pad2)"))
    (pad 24 smd rect (at 4.25 -2.8) (size 1.2 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 25 smd rect (at 2.8 -4.25 90) (size 1.2 0.55) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(R8-Pad2)"))
    (pad 26 smd rect (at 2 -4.25 90) (size 1.2 0.55) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(R25-Pad1)"))
    (pad 27 smd rect (at 1.2 -4.25 90) (size 1.2 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 28 smd rect (at 0.4 -4.25 90) (size 1.2 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 29 smd rect (at -0.4 -4.25 90) (size 1.2 0.55) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(P1-Pad9)"))
    (pad 30 smd rect (at -1.2 -4.25 90) (size 1.2 0.55) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(P1-Pad7)"))
    (pad 31 smd rect (at -2 -4.25 90) (size 1.2 0.55) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(P1-Pad5)"))
    (pad 32 smd rect (at -2.8 -4.25 90) (size 1.2 0.55) (layers F.Cu F.Paste F.Mask))
    (model Housings_QFP.3dshapes/LQFP-32_7x7mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_HC49-SD_SMD (layer F.Cu) (tedit 596CBE4E)
    (at 108.966 87.884 270)
    (descr "Crystal, Quarz, HC49-SD, SMD,")
    (tags "Crystal, Quarz, HC49-SD, SMD,")
    (attr smd)
    (fp_text reference X1 (at -0.127 -3.4036 270) (layer F.SilkS))
    (fp_text value 3.6864MHz (at 0.7874 3.4544 270) (layer F.SilkS))
    (pad 1 smd rect (at -4.84886 0 270) (size 5.6007 2.10058) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad2)"))
    (pad 2 smd rect (at 4.84886 0 270) (size 5.6007 2.10058) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C5-Pad1)"))
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 596CAFF3)
    (at 150.2664 77.3938)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C16 (at 1.524 -1.9812) (layer F.SilkS))
    (fp_text value 470n (at 3.5306 2.1082) (layer F.SilkS))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C16-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 596CBCCF)
    (at 123.19 95.2754)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C17 (at -2.1844 1.9304) (layer F.SilkS))
    (fp_text value 470n (at -0.762 3.4036) (layer F.SilkS))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C17-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 596CBE90)
    (at 127.254 90.3478 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C18 (at 1.3208 1.5748 180) (layer F.SilkS))
    (fp_text value 470n (at -1.4732 1.5748 180) (layer F.SilkS))
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C18-Pad1)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 596CAC63)
    (at 145.3388 70.2818)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 3.1242 2.7432) (layer F.SilkS))
    (fp_text value TEMP_SENS (at 0 -3.1) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 35 "Net-(P2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GNDPWR))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 596CBE80)
    (at 121.2088 91.821 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R31 (at -2.9464 -0.0508 360) (layer F.SilkS))
    (fp_text value 1K (at -2.0828 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(R31-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C17-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 596CBE89)
    (at 125.1712 92.7354)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R32 (at 2.5908 -0.5588) (layer F.SilkS))
    (fp_text value 1K (at 2.286 0.3048) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C17-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C18-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 596CBCB1)
    (at 139.446 93.853 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R15 (at 2.8448 -0.1016 360) (layer F.SilkS))
    (fp_text value 15k (at 3.8608 -0.2032 360) (layer F.SilkS))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C12-Pad1)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965 (layer F.Cu) (tedit 596DF677)
    (at 100.584 70.104)
    (descr "Mounting Hole 3.2mm, no annular, M3, DIN965")
    (tags "mounting hole 3.2mm no annular m3 din965")
    (fp_text reference "" (at -0.889 3.937) (layer F.SilkS))
    (fp_text value "" (at 0 3.8) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965 (layer F.Cu) (tedit 596DE929)
    (at 167.64 141.224)
    (descr "Mounting Hole 3.2mm, no annular, M3, DIN965")
    (tags "mounting hole 3.2mm no annular m3 din965")
    (fp_text reference "" (at 0 -3.8) (layer F.SilkS))
    (fp_text value "" (at 0 3.8) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965 (layer F.Cu) (tedit 5909E202)
    (at 99.949 141.478)
    (descr "Mounting Hole 3.2mm, no annular, M3, DIN965")
    (tags "mounting hole 3.2mm no annular m3 din965")
    (fp_text reference "" (at 0 -3.8) (layer F.SilkS))
    (fp_text value "" (at 0 3.8) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 596CBE68)
    (at 113.2205 79.8195 90)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C7 (at -0.9525 -1.9685 90) (layer F.SilkS))
    (fp_text value 470n (at -4.5085 -0.1905 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 8 +3.3V))
    (pad 2 smd rect (at 1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 596CAFBE)
    (at 139.065 71.501 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at 0 -2.3 270) (layer F.SilkS))
    (fp_text value 470n (at -2.286 1.905 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 +BATT))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 596CBDB4)
    (at 150.368 98.933)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C12 (at -3.81 1.524) (layer F.SilkS))
    (fp_text value 470n (at 0 2.3) (layer F.SilkS))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C12-Pad1)"))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 596CBEAF)
    (at 138.176 88.265 180)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C10 (at 0.254 -1.778 180) (layer F.SilkS))
    (fp_text value 470n (at -2.159 -1.778 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 596CBEB8)
    (at 133.5405 86.0425 90)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at 0.0635 -1.7145 90) (layer F.SilkS))
    (fp_text value 470n (at -0.0635 1.7145 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 596CBEDA)
    (at 128.524 83.312)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C3 (at 1.905 1.778 90) (layer F.SilkS))
    (fp_text value 470n (at 2.794 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ELEKTRONIK:elektra-hexenlogo (layer F.Cu) (tedit 5913451D)
    (at 164.211 81.153)
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 2.54 1.27) (layer F.SilkS) hide)
  )
  (module ELEKTRONIK:Freifunk-Logo (layer F.Cu) (tedit 596CC196)
    (at 163.957 94.107)
    (fp_text reference "" (at 7.62 0) (layer F.SilkS) hide)
    (fp_text value "" (at 7.62 2.54) (layer F.SilkS) hide)
  )
  (module ELEKTRONIK:D_SOD-323_HandSoldering (layer F.Cu) (tedit 596DF295)
    (at 166.497 132.588 270)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D2 (at -3.976 0 270) (layer F.SilkS))
    (fp_text value 1N4001 (at 0.254 -2.159 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 15 VAA))
    (pad 2 smd rect (at 1.25 0 270) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (model Diodes_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module ELEKTRONIK:D_SOD-323_HandSoldering (layer F.Cu) (tedit 596DF348)
    (at 99.314 134.532 270)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D7 (at -3.214 -0.127 270) (layer F.SilkS))
    (fp_text value 1N4001 (at 0.1 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 1.25 0 270) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (model Diodes_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module ELEKTRONIK:D_SOD-323_HandSoldering (layer F.Cu) (tedit 596DF2A0)
    (at 159.258 132.588 270)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D9 (at -3.976 0 270) (layer F.SilkS))
    (fp_text value 1N4001 (at 0.127 -2.032 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 3 +BATT))
    (pad 2 smd rect (at 1.25 0 270) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (model Diodes_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module ELEKTRONIK:DO-214AB (layer F.Cu) (tedit 596E016B)
    (at 121.8565 131.7879 90)
    (descr "Jedec DO-214AB diode package. Designed according to Fairchild SS32 datasheet.")
    (tags "DO-214AB diode")
    (attr smd)
    (fp_text reference D5 (at 0 -4.2 90) (layer F.SilkS))
    (fp_text value DIODESCH (at 0 4.6 90) (layer F.SilkS))
    (pad 2 smd rect (at 3.6 0 90) (size 2.6 3.2) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D5-Pad2)"))
    (pad 1 smd rect (at -3.6 0 90) (size 2.6 3.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (model Diodes_SMD.3dshapes/DO-214AB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58AA84D1)
    (at 101.727 134.874 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C9 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 100n (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58AA84D1)
    (at 128.778 135.382 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C11 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 100n (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 172.974 65.151) (end 172.974 65.278) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_text 1 (at 108.331 74.803) (layer F.SilkS))
  (gr_text "Freifunk-OpenMPPT v1.0" (at 132.969 143.002) (layer F.SilkS))
  (gr_text GND (at 121.158 67.945 90) (layer F.SilkS))
  (gr_text GND (at 118.745 67.818 90) (layer F.SilkS))
  (gr_text GND (at 116.205 67.818 90) (layer F.SilkS))
  (gr_text 3V3 (at 113.665 67.818 90) (layer F.SilkS))
  (gr_text SCL (at 113.538 76.327 90) (layer F.SilkS))
  (gr_text RX (at 118.745 76.073 90) (layer F.SilkS))
  (gr_text TX (at 116.205 75.946 90) (layer F.SilkS))
  (gr_text RST (at 121.285 76.327 90) (layer F.SilkS))
  (gr_text MOSI (at 111.125 76.581 90) (layer F.SilkS))
  (gr_text MISO (at 110.871 67.564 90) (layer F.SilkS))
  (gr_text "Copyright 2017 Corinna 'Elektra' Aichele\nSome component values are preliminary and also depend on the\n voltage range of the MPP tracking required and battery voltage.  \nLicense: Creative Commons - Attribution - ShareAlike 3.0\nhttp://creativecommons.org/licenses/by-sa/3.0/" (at 181.61 172.72) (layer F.Cu))
  (zone (net 3) (net_name +BATT) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 152.527 105.791) (xy 153.543 105.791) (xy 153.543 113.411) (xy 153.67 113.411) (xy 153.67 118.999)
        (xy 157.861 118.999) (xy 157.861 130.937) (xy 159.893 130.937) (xy 159.893 132.207) (xy 157.861 132.207)
        (xy 157.861 132.715) (xy 146.431 132.715) (xy 146.431 102.362) (xy 152.527 102.362)
      )
    )
    (polygon
      (pts        (xy 153.289 113.411) (xy 153.37669 113.411) (xy 153.289 113.344036)
      )
    )
    (polygon
      (pts        (xy 146.431 108.204) (xy 146.558 108.204) (xy 146.558 108.155362)
      )
    )
  )
  (zone (net 2) (net_name GNDPWR) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 167.767 65.7352) (xy 167.64 65.786) (xy 172.593 65.786) (xy 172.593 145.542) (xy 94.996 145.542)
        (xy 94.996 65.786) (xy 97.5868 65.786) (xy 97.7138 65.6844)
      )
    )
  )
  (zone (net 15) (net_name VAA) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 167.639475 101.981) (xy 169.037 101.981) (xy 169.037 132.461) (xy 167.513525 132.461) (xy 167.513 132.588)
        (xy 160.528 132.588) (xy 160.528 130.556) (xy 160.577696 130.565203) (xy 158.369 129.921) (xy 158.369 109.347)
        (xy 160.02 109.347) (xy 160.02 106.553) (xy 156.972 106.553) (xy 156.972 101.854) (xy 167.64 101.854)
      )
    )
  )
  (zone (net 7) (net_name VCC) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 101.092 113.792) (xy 100.33 114.554) (xy 100.203 114.554) (xy 100.203 121.539) (xy 102.108 123.444)
        (xy 110.49 123.444) (xy 110.49 131.699) (xy 100.076 131.699) (xy 100.076 132.969) (xy 98.552 132.969)
        (xy 98.552 131.699) (xy 97.663 131.699) (xy 97.663 120.523) (xy 97.79 120.523) (xy 97.79 119.507)
        (xy 98.425 118.872) (xy 98.425 102.997) (xy 101.092 102.997)
      )
    )
  )
  (zone (net 11) (net_name "Net-(C11-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 145.669 132.08) (xy 144.145 132.08) (xy 144.145 132.207) (xy 131.064 132.207) (xy 130.048 131.191)
        (xy 130.048 113.665) (xy 141.224 113.665) (xy 141.224 102.362) (xy 145.669 102.362)
      )
    )
  )
  (zone (net 16) (net_name "Net-(D5-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 122.174 106.553) (xy 134.366 106.553) (xy 134.874 106.045) (xy 139.573 106.045) (xy 139.573 113.157)
        (xy 129.54 113.157) (xy 129.54 131.445) (xy 111.379 131.445) (xy 111.379 115.443) (xy 109.093 115.443)
        (xy 106.426 112.776) (xy 106.426 112.649) (xy 105.918 112.141) (xy 105.918 105.156) (xy 106.553 104.521)
        (xy 120.142 104.521)
      )
    )
    (polygon
      (pts        (xy 129.54 112.776) (xy 129.54 112.903) (xy 129.667 112.776)
      )
    )
  )
  (zone (net 2) (net_name GNDPWR) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 172.339 145.288) (xy 95.123 145.288) (xy 95.123 65.659) (xy 172.339 65.659)
      )
    )
    (polygon
      (pts        (xy 167.6908 100.965) (xy 167.6908 101.0666) (xy 98.170892 101.570185) (xy 98.171 101.6) (xy 97.409 101.6)
        (xy 97.409 118.491) (xy 96.774 118.491) (xy 96.774 135.382) (xy 103.251 135.382) (xy 103.251 132.588)
        (xy 124.968 132.588) (xy 127.127 134.747) (xy 127.127 135.509) (xy 129.54 135.509) (xy 131.826 133.223)
        (xy 169.926 133.223) (xy 169.926 100.965)
      )
    )
    (polygon
      (pts        (xy 98.044 66.294) (xy 98.044 66.315904) (xy 101.06787 66.294)
      )
    )
  )
  (zone (net 2) (net_name GNDPWR) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 139.319 103.251) (xy 136.144 103.251) (xy 136.144 105.283) (xy 139.319 105.283)
      )
    )
  )
  (zone (net 2) (net_name GNDPWR) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 157.988 107.315) (xy 159.385 107.315) (xy 159.385 108.839) (xy 157.861 108.839) (xy 157.861 107.315)
        (xy 158.115 107.315)
      )
    )
  )
)
